INVITATION FOR QUOTATION

TEQIP-III/2017/nitr/Shopping/2



                       08/12/2017
To,
.

Sub: Invitation for Quotations for supply of Goods

Dear Sir,

1. You are invited to submit your most competitive quotation for the following goods with item wise detailed specifications given at Annexure I,
	Sr. No
	Brief Description
	Quantity
	Delivery Period(In days)
	Place of Delivery
	Installation Requirement (if any)

	1
	Multi Electrode Resistivity Imaging System
	1
	60
	Department of Applied Geology, National Institute of Technology , Raipur, Chhattisgarh,492001
	Yes


2. Government of India has received a credit from the International Development Association (IDA) towards the cost of the Technical Education Quality Improvement Programme[TEQIP]-Phase II Project and intends to apply part of the proceeds of this credit to eligible payments under the contract for which this invitation for quotations is issued.
3. Quotation,
3.1 The contract shall be for the full quantity as described above. 
3.2 Corrections, if any, shall be made by crossing out, initialing, dating and re writing.
3.3 All duties and other levies payable by the supplier under the contract shall be included in the unit price.
3.4 Applicable taxes shall be quoted separately for all items.
3.5 The prices quoted by the bidder shall be fixed for the duration of the contract and shall not be subject to adjustment on any account.
3.6 The Prices should be quoted in Indian Rupees only.
4. Each bidder shall submit only one quotation.

5. Quotation shall remain valid for a period not less than 55 days after the last date of quotation submission.

6. Evaluation of Quotations,
The Purchaser will evaluate and compare the quotations determined to be substantially responsive i.e. which

6.1 are properly signed ; and
6.2 confirm to the terms and conditions, and specifications.
6.3 The Tenderer / Bidder need to submit the following certificates along with the quotation to   

  * Confirm their eligibility:

* Proof of establishment of Firms/shop/business/manufacturing unit etc. and Dealership   certificate from the principals etc.

* GST certificate should be enclosed

*Previous Purchase order copy of the same item.
7. The Quotations would be evaluated for all items together.

8. Award of contract: 

The Purchaser will award the contract to the bidder whose quotation has been determined to be substantially responsive and who has offered the lowest evaluated quotation price.

8.1 Notwithstanding the above, the Purchaser reserves the right to accept or reject any quotations and to cancel the bidding process and reject all quotations at any time prior to the award of contract.

8.2 The bidder whose bid is accepted will be notified of the award of contract by the Purchaser prior to expiration of the quotation validity period. The terms of the accepted offer shall be incorporated in the purchase order.
9. Payment shall be made in Indian Rupees as follows:
	Delivery and Installation – 0% of total cost
Satisfactory Acceptance - 100% of total cost


10. All supplied items are under warranty of 12 months from the date of successful acceptance of items.
11. You are requested to provide your offer latest by 15:00 hours on 08.01.2018

12. Detailed specifications of the items are at Annexure I.
13. Training Clause (if any) Yes
14. Testing/Installation Clause (if any) Yes
15. Information brochures/ Product catalogue, if any must be accompanied with the quotation clearly indicating the model quoted for. 

16. Sealed quotation to be submitted/ delivered at the address mentioned below,
   Registrar,
  National Institute of Technology,
   G.E, Road, Raipur,

         Chhattisgarh, Pin code-492001
17. We look forward to receiving your quotation and thank you for your interest in this project.

REGISTRAR

NIT RAIPUR
                                                                   Annexure I
	Sr. No
	Item Name
	                   Specifications

	I
	Multi Electrode Resistivity Imaging System
	A

	
	
	01
	General description of equipment 
	The main processing unit should be compact and light weight with LCD/LED display (Color and day light visible), microprocessor controlled, Internal memory and multi-electrodes (72 electrodes) system are integrated in the same housing in single equipment. Automatic injection current ranging, stacking and averaging. No electronic devices in-between the cables. 

	
	
	02
	Electrodes Arrays 
	Main unit should be configured for at least Wenner, Schlumberger, Gradient, Dipole-dipole arrays. Enable to take up to maximum possible depth penetration of current during Imaging survey by above configuration by 72 electrodes. 

	
	
	03
	No. of Channel 
	10 channels or more 

	
	
	04
	Cable 
	Multi core 72 takes out in 10 m spacing 

	
	
	05
	Data transfer 
	Equipment can be interfaced with PC or laptop for upload and load of Sequence file and data file 

	
	
	06
	Memory Capacity 
	Minimum 40,000 readings 

	
	
	07
	Power source 
	12/24 Volts re-chargeable battery source for imaging, data acquisition and data transfer to external PC/Laptop and external power source for 96 Volts or more for the booster for deep penetration

	
	
	08
	Output transmitting Power 
	250 W or more

	
	
	09
	Output current maximum 
	2.5A or more

	
	
	10
	Output Voltage 
	800 V or more (Peak to Peak 1200 V or more)

	
	
	11
	Automatic Ranging 
	Microprocessor controlled 

	
	
	12
	Measurement 
	Direct measurement of Resistivity, SP and IP 

	
	
	13
	Current measurement precession 
	0.2 percent typical or better 

	
	
	14
	Resistivity accuracy 
	0.2 percent typical or better 

	
	
	15
	Voltage 

measurement / precision 


	0.2 % typical / 1 micro-Volt or better 

	
	
	16
	Input Impedance
	100 Mega Ohm or better

	
	
	17
	Input Voltage protection 
	Up-to 1000V or better 

	
	
	18
	GPS
	The unit should have the inbuilt GPS system

	
	
	19
	Noise Reduction 
	Continuous stacking selectable automatic. Noise should be monitored automatically before injection of current 

	
	
	20
	SP compensation 
	Through automatic linear drift correction. 

	
	
	21
	Induced Polarization 
	Arbitrary windows flexibility, configured to power line frequencies 

	
	
	22
	Measurement method 
	Roll along facility, move sequence 

	
	
	23
	Environmental 
	Weather proof, Shock proof 

	
	
	24
	Operating Temp 
	All weather temperature of Indian tropical and cold climatic condition 
(-50C to 550C) 

	
	
	25
	Dedicated Software 
	Sequence creation, data acquisition, data transfer, processing, filtering, 2D/3D inversion and interpretation etc. 

	
	
	                                                              B

	
	
	Data transfer, processing &interpretation device

	Compatible Laptop for data transfer, processing & interpretation, latest Window operating system (Not less than Window-10), 1 TB HDD, 8 GB RAM, 04 GB Graphic Card, latest microprocessor (Core i7), size


	
	
	C. Scheduled requirement (Complete set of equipment with software, Laptop, accessories etc.):
1. 10 Channel, 72 Electrode Resistivity/ IP Imaging system: 1 unit 

2. Multi Core Cable with 72 take-outs with 10 m spacing: 1 set 

3. Stain steel electrodes with connector to cable :80 No’s 

4. Jumpers, data transfer cable, connector etc.: 1 set 

5. 12/24 rechargeable Battery with all leads and Charger: 1 set 

6. Software for sequence creation, data acquisition, data transfer 2D/3D inversion and 

interpretation (With License): 1 No 

7. Rugged Laptop for data processing with required software with license: 1 No 

8. Tool Kits(Digital multi-meter, nose pliers, wire cutter, screw driver, etc): 1set 

9. Test box for Resistance: 1 no 

10. Leaflet and Brochures: Operation, maintenance as well as software’s: 1 set


	
	
	D. Training: 
Training by trained person for data acquisition, processing, interpretation, up keep and maintenance and trouble shooting, field minor repairing, principle as well as practical to faculty members/ students for five working days at supplier cost.


	
	
	E. Installation, commissioning and field testing: 
Supplier has to arrange for commissioning and testing of Resistivity Imaging units along with its components at jurisdiction of consignee place at supplier cost. Commissioning and field testing should be arranged within 10 days from date of intimation by NIT Raipur.



                                                                     FORMAT FOR QUOTATION SUBMISSION

(In letterhead of the supplier with seal)

                                                                                                                                                                             Date: _______________
To: 






____________________________

____________________________

                                                                                                                                          GST No…………………………………                 

	Sl. No.
	Description of goods (with full Specifications)
	Qty.
	Unit
	Quoted Unit rate in Rs.

(Including Ex Factory price, excise duty, packing and forwarding, transportation, insurance, other local costs incidental to delivery and warranty/ guaranty commitments) 
	Total Price 

(A)
	                        GST 

	
	
	
	
	
	
	  GST  taxes mentioned as under 
	Percentage (%)
	In figures (B)

	
	
	
	
	
	
	CGST
	
	

	
	
	
	
	
	
	SGST
	
	

	
	
	
	
	
	
	IGST
	
	

	Total Cost
	
	Total 
	
	


Gross Total Cost (A+B): Rs. ________________

We agree to supply the above goods in accordance with the technical specifications for a total contract price of Rs. ———————— (Amount in figures) (Rupees ————————amount in words) within the period specified in the Invitation for Quotations.

We confirm that the normal commercial warranty/ guarantee of ——————— months shall apply to the offered items and we also confirm to agree with terms and conditions as mentioned in the Invitation Letter. 

We hereby certify that we have taken steps to ensure that no person acting for us or on our behalf will engage in bribery.

Signature of Supplier

Name: __________________

Address: __________________

Contact No: ______________
