INVITATION FOR QUOTATION

TEQIP-III/2018/nitr/Shopping/24



                       19-Feb-2018
To,

Sub: Invitation for Quotations for supply of Goods

Dear Sir,

1. You are invited to submit your most competitive quotation for the following goods with item wise detailed specifications given at Annexure I,
	Sr. No
	Brief Description
	Quantity
	Delivery Period(In days)
	Place of Delivery
	Installation Requirement (if any)

	1
	Deep Learning Machine-Devbox
	2
	60
	Department of Computer Science,  National Institute of Technology,  Raipur, Chhattisgarh 492010
	yes


2. Government of India has received a credit from the International Development Association (IDA) towards the cost of the Technical Education Quality Improvement Programme[TEQIP]-Phase III Project and intends to apply part of the proceeds of this credit to eligible payments under the contract for which this invitation for quotations is issued.

3. Quotation,
3.1 The contract shall be for the full quantity as described above. 
3.2 Corrections, if any, shall be made by crossing out, initialing, dating and re writing.
3.3 All duties and other levies payable by the supplier under the contract shall be included in the unit price.
3.4 Applicable taxes shall be quoted separately for all items.
3.5 The prices quoted by the bidder shall be fixed for the duration of the contract and shall not be subject to adjustment on any account.
3.6 The Prices should be quoted in Indian Rupees only.
4. Each bidder shall submit only one quotation.

5. Quotation shall remain valid for a period not less than 55 days after the last date of quotation submission.

6. Evaluation of Quotations,
The Purchaser will evaluate and compare the quotations determined to be substantially responsive i.e. which

6.1 are properly signed ; and
6.2 confirm to the terms and conditions, and specifications.
6.3 The Tenderer / Bidder need to submit the following certificates along with the quotation to   
  * Confirm their eligibility:
* Proof of establishment of Firms/shop/business/manufacturing unit etc. and Dealership   certificate from the principals etc.

* GST certificate  should be enclosed
*Previous Purchase order copy
7. The Quotations would be evaluated for all items together.

8. Award of contract: 

The Purchaser will award the contract to the bidder whose quotation has been determined to be substantially responsive and who has offered the lowest evaluated quotation price.

8.1 Notwithstanding the above, the Purchaser reserves the right to accept or reject any quotations and to cancel the bidding process and reject all quotations at any time prior to the award of contract.

8.2 The bidder whose bid is accepted will be notified of the award of contract by the Purchaser prior to expiration of the quotation validity period. The terms of the accepted offer shall be incorporated in the purchase order.
9. Payment shall be made in Indian Rupees as follows:
	Delivery and Installation - 0% of total cost
Satisfactory Acceptance - 100% of total cost


10. All supplied items are under warranty of 36 months from the date of successful acceptance of items.
11. You are requested to provide your offer latest by 15:00 hours on 20-Mar-2018 .
12. Detailed specifications of the items are at Annexure I.
13. Training Clause (if any) Yes
14. Testing/Installation Clause (if any) Yes
15. Information brochures/ Product catalogue, if any must be accompanied with the quotation clearly indicating the model quoted for. 

16. Sealed quotation to be submitted/ delivered at the address mentioned below,
National Institute of Technology, Raipur
17. We look forward to receiving your quotation and thank you for your interest in this project.

REGISTRAR

NIT RAIPUR
                                                                      Annexure I
	Sr. No
	Item Name
	Specifications

	1
	Deep Learning Machine /Devbox
	Characteristic 
	Computational Node - Quantity 2

	
	
	Processor
	Motherboard must be capable of supporting up to two Intel® Xeon® Processor SP, up to 28 cores per processor; to be supplied with 2 x Intel® Xeon®  Silver 4110 Processor (11M Cache, 2.10 GHz)

	
	
	Memory
	24 DDR4 DIMM slots, Supports RDIMM / LRDIMM, speeds up to Memory 2666MT/s, 3TB max, to be supplied with 8 x 32 GB registered ECC  DDR4 2666 DIMMs

	
	
	Storage controllers: 
	Internal controllers: 12 Gbps RAID controller with 1 GB flash-backed cache

	
	
	Drive bays
	Front drive bays: Up to 8 x 2.5” SAS/SATA (HDD/SSD) max 61TB, to be supplied with 3 x 1.2 TB 10K rpm SAS, Internal DVD+RW

	
	
	Hard Disk
	4 TB (minimum) 7200 RPM

	
	
	GPU accelerator
	1 x NVIDIA® Tesla® 16 GB P100 GPU accelerator or High, offered system 

GPU accelerator 

should support additional GPU accelerator as future upgrade, all 

necessary cables, mounting kit accessories etc. should be present from   day 1   

	
	
	Power supplies
	Platinum 1200W (minimum), Hot plug power supplies with full 

redundancy, Up to 6 hot plugs fans with full redundancy

	
	
	Sizing 
	Form factor : Rack (2U)   

	
	
	Embedded management
	IPMI 2.0 compliant, remote / virtual media & video redirection, GUI,  RESTful API integration, event management, threshold management, Embedded asset management, performance management, fault management management with predictive self-healing, monitoring & power control consumption  with history for at least 1 year, drivers & BIOS firmware should be  available for free even after the warranty for the server is over

	
	
	I/O & Ports
	Network daughter card options  2 x 10GE + 2 x 1GE  Front ports: 2 x USB 3.0 

I/O & Ports 

Rear ports: Video, 2 x USB 3.0, dedicated 1 GE network management 

port   Internal ports: 1 x USB 3.0  3 PCIe Gen 3 x16 slots, 3 PCIe Gen 3 x8 slots, integrated on  motherboard without the use of riser cards

	
	
	Supported 


	Canonical® Ubuntu® LTS 
Citrix® XenServer® 

Microsoft Windows Server® with Hyper-V 

operating Red Hat® Enterprise Linux systems 

SUSE® Linux Enterprise Server   VMware® ESXi

	
	
	Operating System
	To be supplied with Canonical® Ubuntu® 16.04 LTS 64-bit, offered System model must be listed on https://certification.ubuntu.com/server/ Compliance

	
	
	Compliance
	BIS, CE, CSA, FCC Class A, ASHRAE Class A3, RoHS

	
	
	Warranty 


	3 years comprehensive OEM Onsite warranty with Next Business Day 

resolution

	
	
	Remote Collaboration System
	It should support One to One for remote work and One to many for Collaboration with keyboard and mouse control. Solution - Should work on both Linux and Windows, and should be inter-operable.    - It should allow collaboration between multiple participants on an  OpenGL 3D or DirectX applications


FORMAT FOR QUOTATION SUBMISSION

(In letterhead of the supplier with seal)

                                                                                                                                                                                                           Date: _______________
To: 






____________________________

____________________________

	Sl. No.
	Description of goods (with full Specifications)
	Qty.
	Unit
	Quoted Unit rate in Rs.

(Including Ex Factory price, excise duty, packing and forwarding, transportation, insurance, other local costs incidental to delivery and warranty/ guaranty commitments) 
	Total Price 

(A)
	                        GST 

	
	
	
	
	
	
	  GST  taxes mentioned as under 
	Percentage (%)
	In figures (B)

	
	
	
	
	
	
	CGST
	
	

	
	
	
	
	
	
	SGST
	
	

	
	
	
	
	
	
	IGST
	
	

	Total Cost
	
	Total 
	
	


Gross Total Cost (A+B): Rs. ________________

We agree to supply the above goods in accordance with the technical specifications for a total contract price of Rs. ———————— (Amount in figures) (Rupees ————————amount in words) within the period specified in the Invitation for Quotations.

We confirm that the normal commercial warranty/ guarantee of ——————— months shall apply to the offered items and we also confirm to agree with terms and conditions as mentioned in the Invitation Letter. 

We hereby certify that we have taken steps to ensure that no person acting for us or on our behalf will engage in bribery.

Signature of Supplier

Name: __________________

Address: __________________

Contact No: ______________
